#
# This is a sample of the file tnn.ini with all options and devices shown.
#
#-----------------------------------------------------------------------------
#
# Average rounds/sec (default if missing is 100) - the real value depends
# on processor power and system load. Increase this on heavy loaded systems
# and if you have high speed ports (76800 baud and up). Normally, it doesn't
# need to be changed, if more power is required, tnn increases rounds by
# itself. This value can be interpreted as some kind of idle gas ;)
#
#rounds 200
#
# File permissions for files created by TNN - octal value as used by umask(2)
# default value is 000 (world readable/writable & EXECUTEABLE !!!).
# use 077 to limit access to the owner of TNN only (suggested)
#
#perms 077
#
# Working directory for TNN
#
tnn_dir /usr/local/tnn/
#
# Unix-Socket for TNNs hostmode interface (optional)
#
#tnn_socket /usr/local/tnn/tnn-socket
#
# Program to start before using any hardware ports (optional) - don't use
# any parameters!
#
#tnn_start kill_other_processes
#
# Number of buffers (optional; default = 10000)
#
buffers 10000
#
# File containing process id (mandatory)
#
tnn_procfile tnn.pid
#
#-----------------------------------------------------------------------------
# Example Device Configurations
#-----------------------------------------------------------------------------
# device 1 = Tokenring on /dev/ttyS0; 38400 Bd; Ports 0 and 1
device /dev/ttyS0
# lockfile for device 1
tnn_lockfile /var/lock/LCK..ttyS0
# speed on device 1
speed 38400
# type of KISS on device 1:
# 0 = KISS, 1 = SMACK, 2 = RMNC-KISS, 3 = Tokenring (1st device only),
# 4 = Vanessa, 5 = SCC, 6 = TF (experimental!), 7 = IPX (1 IPX port only),
# 8 = AX25IP (1 AX25IP port only), 9 = Loop, 10 = Kernel-AX.25 Interface
# 11 = Kernel-AX.25 Interface for DG1KJD-Kernel, 12 = 6PACK
#
# 22 = Telnet, 23 = Httpd, 24 = IPConvers
kisstype 3
# L2-Port(s) associated with device 1 - use several port lines, one for every
# TNC in your tokenring. The ports assigned here MUST match the TNC-number
# burned into the ROM of the tokenring-TNC !!!
port 0
port 1
#-----------------------------------------------------------------------------
# device 2 = standard KISS on /dev/ttyS1; 9600Bd; Port 2
device /dev/ttyS1
# lockfile for device 2
tnn_lockfile /var/lock/LCK..ttyS1
# speed on device 2
speed 9600
# type of KISS on device 2:
# 0 = KISS, 1 = SMACK, 2 = RMNC-KISS,
# 4 = Vanessa, 5 = SCC, 6 = TF (experimental!), 7 = IPX (1 IPX port only),
# 8 = AX25IP (1 AX25IP port only), 9 = Loop, 10 = Kernel-AX.25 Interface
# 11 = Kernel-AX.25 Interface for DG1KJD-Kernel, 12 = 6PACK
#
# 22 = Telnet, 23 = Httpd, 24 = IPConvers
kisstype 0
# L2-Port associated with device 2
port 2
#-----------------------------------------------------------------------------
# device 3 = SMACK on /dev/ttyS2; 115200 Bd; Port 3
device /dev/ttyS2
# lockfile for device 3
tnn_lockfile /var/lock/LCK..ttyS2
# speed on device 3
speed 115200
# type of KISS on device 3:
# 0 = KISS, 1 = SMACK, 2 = RMNC-KISS,
# 4 = Vanessa, 5 = SCC, 6 = TF (experimental!), 7 = IPX (1 IPX port only),
# 8 = AX25IP (1 AX25IP port only), 9 = Loop, 10 = Kernel-AX.25 Interface
# 11 = Kernel-AX.25 Interface for DG1KJD-Kernel, 12 = 6PACK
#
# 22 = Telnet, 23 = Httpd, 24 = IPConvers
kisstype 1
# L2-Port associated with device 3
port 3
#-----------------------------------------------------------------------------
# device 4 = RMNC-Kiss on /dev/ttyS3; 19200 Bd; Port 4
device /dev/ttyS3
# lockfile for device 4
tnn_lockfile /var/lock/LCK..ttyS3
# speed on device 4
speed 19200
# type of KISS on device 4:
# 0 = KISS, 1 = SMACK, 2 = RMNC-KISS,
# 4 = Vanessa, 5 = SCC, 6 = TF (experimental!), 7 = IPX (1 IPX port only),
# 8 = AX25IP (1 AX25IP port only), 9 = Loop, 10 = Kernel-AX.25 Interface
# 11 = Kernel-AX.25 Interface for DG1KJD-Kernel, 12 = 6PACK
#
# 22 = Telnet, 23 = Httpd, 24 = IPConvers
kisstype 2
# L2-Port associated with device 4
port 4
#-----------------------------------------------------------------------------
# device 5 = VANESSA-Board ; Port 5
device Vanessa
#
# no "tnn_lockfile"- or "speed"-lines required here!
#
# type of KISS on device 5:
# 0 = KISS, 1 = SMACK, 2 = RMNC-KISS,
# 4 = Vanessa, 5 = SCC, 6 = TF (experimental!), 7 = IPX (1 IPX port only),
# 8 = AX25IP (1 AX25IP port only), 9 = Loop, 10 = Kernel-AX.25 Interface
# 11 = Kernel-AX.25 Interface for DG1KJD-Kernel, 12 = 6PACK
#
# 22 = Telnet, 23 = Httpd, 24 = IPConvers
kisstype 4
# L2-Port associated with device 5
port 5
#-----------------------------------------------------------------------------
# device 6 = SCC on /dev/scc0; Port 6
device /dev/scc0
# lockfile for device 6
tnn_lockfile /var/lock/LCK..scc0
# type of KISS on device 6:
# 0 = KISS, 1 = SMACK, 2 = RMNC-KISS,
# 4 = Vanessa, 5 = SCC, 6 = TF (experimental!), 7 = IPX (1 IPX port only),
# 8 = AX25IP (1 AX25IP port only), 9 = Loop, 10 = Kernel-AX.25 Interface
# 11 = Kernel-AX.25 Interface for DG1KJD-Kernel, 12 = 6PACK
#
# 22 = Telnet, 23 = Httpd, 24 = IPConvers
kisstype 5
# L2-Port associated with device 6
port 6
#-----------------------------------------------------------------------------
# device 7 = TNC with TF 2.7b/KISS on /dev/ttyS4; 19200 Bd; Port 7
# WARNING! This configuration is NOT recommended for a standalone digipeater!
device /dev/ttyS4
# lockfile for device 7
tnn_lockfile /var/lock/LCK..ttyS4
# speed on device 7
speed 19200
# type of KISS on device 7:
# 0 = KISS, 1 = SMACK, 2 = RMNC-KISS,
# 4 = Vanessa, 5 = SCC, 6 = TF (experimental!), 7 = IPX (1 IPX port only),
# 8 = AX25IP (1 AX25IP port only), 9 = Loop, 10 = Kernel-AX.25 Interface
# 11 = Kernel-AX.25 Interface for DG1KJD-Kernel, 12 = 6PACK
#
# 22 = Telnet, 23 = Httpd, 24 = IPConvers
kisstype 6
# L2-Port associated with device 7
port 7
#-----------------------------------------------------------------------------
# device 8 = AX25IPX ; Port 8
device ipx
# type of KISS on device 8:
# 0 = KISS, 1 = SMACK, 2 = RMNC-KISS,
# 4 = Vanessa, 5 = SCC, 6 = TF (experimental!), 7 = IPX (1 IPX port only),
# 8 = AX25IP (1 AX25IP port only), 9 = Loop, 10 = Kernel-AX.25 Interface
# 11 = Kernel-AX.25 Interface for DG1KJD-Kernel, 12 = 6PACK
#
# 22 = Telnet, 23 = Httpd, 24 = IPConvers
kisstype 7
# L2-Port associated with device 8
port 8
#-----------------------------------------------------------------------------
# device 9 = AX25IP ; Port 9
device ax25ip
# type of KISS on device 9:
# 0 = KISS, 1 = SMACK, 2 = RMNC-KISS,
# 4 = Vanessa, 5 = SCC, 6 = TF (experimental!), 7 = IPX (1 IPX port only),
# 8 = AX25IP (1 AX25IP port only), 9 = Loop, 10 = Kernel-AX.25 Interface
# 11 = Kernel-AX.25 Interface for DG1KJD-Kernel, 12 = 6PACK
#
# 22 = Telnet, 23 = Httpd, 24 = IPConvers
kisstype 8
# L2-Port associated with device 9
port 9
#-----------------------------------------------------------------------------
# device 10 = Kernel-AX.25; Port 10 (example with Interface ax0)
device ax0
# type of KISS on device 10:
# 0 = KISS, 1 = SMACK, 2 = RMNC-KISS,
# 4 = Vanessa, 5 = SCC, 6 = TF (experimental!), 7 = IPX (1 IPX port only),
# 8 = AX25IP (1 AX25IP port only), 9 = Loop, 10 = Kernel-AX.25 Interface
# 11 = Kernel-AX.25 Interface for DG1KJD-Kernel, 12 = 6PACK
#
# 22 = Telnet, 23 = Httpd, 24 = IPConvers
kisstype 10
# L2-Port associated with device 10
port 10
#-----------------------------------------------------------------------------
# device 11 = DG1KJD-Kernel-AX.25; Port 11 (example with Interface ax0)
device ax0
# type of KISS on device 11:
# 0 = KISS, 1 = SMACK, 2 = RMNC-KISS,
# 4 = Vanessa, 5 = SCC, 6 = TF (experimental!), 7 = IPX (1 IPX port only),
# 8 = AX25IP (1 AX25IP port only), 9 = Loop, 10 = Kernel-AX.25 Interface
# 11 = Kernel-AX.25 Interface for DG1KJD-Kernel, 12 = 6PACK
#
# 22 = Telnet, 23 = Httpd, 24 = IPConvers
kisstype 11
# L2-Port associated with device 11
port 11
#-----------------------------------------------------------------------------
# device 12 = 6PACK TNC(s) on /dev/ttyS5; 57600 Bd; Ports 12 and 13
device /dev/ttyS5
# lockfile for device 1
tnn_lockfile /var/lock/LCK..ttyS5
# speed on device 1
speed 57600
# type of KISS on device 1:
# 0 = KISS, 1 = SMACK, 2 = RMNC-KISS, 3 = Tokenring (1st device only),
# 4 = Vanessa, 5 = SCC, 6 = TF (experimental!), 7 = IPX (1 IPX port only),
# 8 = AX25IP (1 AX25IP port only), 9 = Loop, 10 = Kernel-AX.25 Interface
# 11 = Kernel-AX.25 Interface for DG1KJD-Kernel, 12 = 6PACK
#
# 22 = Telnet, 23 = Httpd, 24 = IPConvers
kisstype 12
# L2-Port(s) associated with device 12 - use several port lines, one for every
# TNC in the 6PACK-ring. The ring is auto-configured at startup, the first
# port found here is assigned to the first TNC in the ring, the second port to
# the second TNC and so on. The maximum of TNCs in a 6PACK-ring is 8 !
#
# If you wish to attach more than one 6PACK-TNC, you *MUST* build a ring !
# It is not possible to have more than one device configured as 6PACK at
# the moment ! This is a new device, if you find errors, please report them !!!
#
port 12
port 13
#-----------------------------------------------------------------------------
# device 22 = TELNET on TCP-Port 23
device 23
# type of KISS on device 1:
# 0 = KISS, 1 = SMACK, 2 = RMNC-KISS, 3 = Tokenring (1st device only),
# 4 = Vanessa, 5 = SCC, 6 = TF (experimental!), 7 = IPX (1 IPX port only),
# 8 = AX25IP (1 AX25IP port only), 9 = Loop, 10 = Kernel-AX.25 Interface
# 11 = Kernel-AX.25 Interface for DG1KJD-Kernel, 12 = 6PACK
#
# 22 = Telnet, 23 = Httpd, 24 = IPConvers
kisstype 22
# L2-Port associated with device 15
port 15
#
# END